TRUESPOKE WHEEL WASHER
INSTALLATION GUIDE
Please read before installation
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IMPORTANT WASHER ORIENTATION
The supplied washers are stamped "WHEEL SIDE". Install each washer with the side marked "WHEEL SIDE" facing downward toward the wheel hub, as shown in the photos above.

WARNING
Never use an air wrench or other power tool to tighten lug nuts. Excessive torque can damage chrome plating and may void your chrome warranty. Tighten lug nuts by hand using a calibrated torque wrench only.
	Thread Pattern
	Torque Specification

	7/16 inch
	75 ft-lbs

	1/2 inch
	85 ft-lbs

	12 mm
	70 ft-lbs



Technical support is always a phone call or email away. Thank you for your business.
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Motorspot, Inc.
427 Industrial Way, Unit C
Fallbrook, California 92028
760-731-8303
